[bookmark: 参数注册表（中文）]参数注册表（中文）




[bookmark: Meta]Meta




	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
meta.case_name
	无
	模板层
	全部
	是
	显示名称

	
meta.case_id
	无
	模板层
	全部
	是
	稳定的预设 ID

	
meta.description
	无
	模板层
	全部
	是
	自由文本描述

	
meta.source_case_folder
	文件夹名
	模板层
	全部
	否
	用于追踪来源

	
meta.created_from_template
	无
	模板层
	全部
	否
	预设来源

	
meta.version
	无
	配置系统
	全部
	否
	Schema 版本



[bookmark: Model]Model

	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
model.modelflag
	
modelflag
	
main1.m
	1-7
	是
	当前算例均使用 1

	
model.grid_model
	
grid_model
	
main1.m
	1-7
	是
	1 为 SP， 2 为 DP

	
model.flow_model
	
flow_model
	
main1.m
	1-7
	是
	1 气 水 ， 2 油 水 ， 3 组 分 流


[bookmark: Grid Geometry]Grid Geometry

	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
grid.dx
	
dx
	
main1.m
	1-7
	是
	向量

	
grid.dy
	
dy
	
main1.m
	1-7
	是
	向量

	
grid.dz
	
dz
	
main1.m
	1-7
	是
	向量

	
grid.nx
	
nx
	
main1.m
	1-7
	否
	由 dx 推 导

	
grid.ny
	
ny
	
main1.m
	1-7
	否
	由 dy 推 导

	
grid.nz
	
nz
	
main1.m
	1-7
	否
	由 dz 推 导

	
grid.NTG
	
NTG
	
main1.m
	1-7
	否
	大小为 nx*ny*nz 的数组



由 GridProp_pre.m 生成的派生字段：

	grid.coordinates
	

	grid.nodes
	

	grid.nP
	

	grid.nmc
	

	grid.dxv
	

	grid.dyv
	

	grid.dzv
	

	grid.zm
	

	grid.vm
	

	grid.xrao
	

	grid.yrao
	

	grid.zrao
	

	grid.cell_mid_coords



[bookmark: Fracture Input]Fracture Input

	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
fracture. input_style
	
input_style
	
main1.m
	1-7
	是
	1 工程输入，2 向量输入，3 二维线段输入，4 fab 预留

	
fracture. input_content
	
input_content
	
main1.m
	1-7
	是
	工程裂缝表

	
fracture.f
	
f
	main1.m / helper 输出
	1-7
	高级
	裂缝向量表示



	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
fracture.fellip
	
fellip
	main1.m / helper 输出
	1-7
	高级
	椭圆裂缝

	
fracture. fractureLines
	
fractureLines
	
main1.m
	1-7
	是
	在模式 3 下使用

	
fracture. fractureHeights
	
fractureHeights
	
main1.m
	1-7
	是
	在模式 3 下使用

	
fracture. flowBarrierFlags
	
flowBarrierFlags
	
main1.m
	1-7
	是
	可选

	
fracture. frac_information
	
frac_information
	helper 输出
	1-7
	否
	由辅助函数生成

	
fracture.nf
	
nf
	
main1.m
	1-7
	否
	裂缝数量派生值



[bookmark: Discretization Selection]Discretization Selection

	
Config Path
	Source Variable
	Source File
	
Cases
	
Editable
	
Notes

	
discretization.mode
	
grid_model
	
main1.m
	1-7
	是
	与 model.grid_model 对应

	
discretization.use_operator
	隐式
	
main1.m
	1-7
	否
	当前始终调用 OperatorRS


[bookmark: SP Rock And Boundary Parameters]SP Rock And Boundary Parameters
 (
discretization.
sp.
boundary_polygon
)这些字段是关键的可编辑参数，之前统计时偏少。

	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
	
boundary
	
grid_discretization_SP_model. m
	1
	是
	不规则计算域边界多边形
	



	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
discretization. sp.invalid_layer
	
invalid_layer
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	在模拟中禁用的层号

	
discretization. sp.valid_grids
	
valid_grids
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	否
	由边界和层信息推导
	

	
discretization. sp.matrix.kx
	
kx
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	数组或生成场

	
discretization. sp.matrix.ky
	
ky
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	数组或生成场
	

	
discretization. sp.matrix.kz
	
kz
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	数组或生成场

	
discretization. sp.matrix.pori
	
pori
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	数组或生成场
	

	
discretization. sp.matrix.prpor
	
prpor
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	基质参考压力

	
discretization. sp.matrix.cpor
	
cpor
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	基质压缩系数
	

	
discretization. sp.matrix. rock_density
	rock_density /
density_rock
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	各算例命名不一致

	
discretization. sp.fracture.Kf
	
Kf
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	裂缝渗透率
	

	
discretization.
	
Wf
	
	1,2,4,5,6,7
	是
	裂缝




	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
sp.fracture.Wf
	
	
grid_discretization_SP_model. m
	
	
	缝宽

	
discretization. sp.fracture.
Porf
	
Porf
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	裂缝孔隙度
	

	
discretization. sp.fracture. prporf
	
prporf
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	裂缝参考压力

	
discretization. sp.fracture. cporf
	
cporf
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	裂缝压缩系数
	

	
discretization. sp.stress. fracture_factor
	
stress_factor_fracture
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	应力敏感系数

	
discretization. sp.stress. matrix_factor
	
stress_factor_matrix
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	应力敏感系数
	

	
discretization. sp.stress. ref_pressure
	
stress_factor_ref_pressure
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	参考压力

	
discretization. sp.stress.Rpt
	
Rpt
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	含义待进一步确认
	

	
discretization. sp.stress.cf
	
cf
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	含义待进一步确认

	
discretization. sp.stress.ca
	
ca
	
grid_discretization_SP_model. m
	1,2,4,5,6,7
	是
	含义待进一步确认
	



各算例补充说明：
算例 1 使用空间函数和不规则多边形边界。

算例 2 和 4 在适用时使用

invalid_layer

关闭第二层。

算例 5 和 7 的常数基质参数与算例 2、4、6 不同。

[bookmark: DP Rock Parameters]DP Rock Parameters

	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
discretization. dp. fracture_layer. kx
	
kx
	
grid_discretization_DP_model. m
	3
	是
	双重介质中的裂缝层

	
discretization. dp. fracture_layer. ky
	
ky
	
grid_discretization_DP_model. m
	3
	是
	双重介质中的裂缝层

	
discretization. dp. fracture_layer. kz
	
kz
	
grid_discretization_DP_model. m
	3
	是
	双重介质中的裂缝层

	
discretization. dp. fracture_layer. pori
	
pori
	
grid_discretization_DP_model. m
	3
	否
	裂缝层孔隙度

	
discretization. dp.matrix_layer. kx
	
kx_matrixLayer
	
grid_discretization_DP_model. m
	3
	是
	基质层渗透率

	
discretization. dp.matrix_layer. ky
	
ky_matrixLayer
	
grid_discretization_DP_model. m
	3
	是
	基质层渗透率

	
discretization. dp.matrix_layer. kz
	
kz_matrixLayer
	
grid_discretization_DP_model. m
	3
	是
	基质层渗透率

	
discretization. dp.matrix_layer. pori
	
pori_matrixLayer
	
grid_discretization_DP_model. m
	3
	是
	基质层孔隙度

	
discretization. dp.shape_factor
	
sigma
	
grid_discretization_DP_model. m
	3
	是
	孔隙间形状因子

	
discretization.
	
valid_grids
	
	3
	否
	当前算



	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
dp.valid_grids
	
	
grid_discretization_DP_model. m
	
	
	例中全为 1

	
discretization. dp.NTG
	
NTG
	
grid_discretization_DP_model. m
	3
	是
	在文件中被重新赋值

	
discretization. dp.prpor
	
prpor
	
grid_discretization_DP_model. m
	3
	是
	参考压力

	
discretization. dp.cpor
	
cpor
	
grid_discretization_DP_model. m
	3
	是
	压缩系数

	
discretization. dp.fracture.Kf
	
Kf
	
grid_discretization_DP_model. m
	3
	是
	裂缝渗透率

	
discretization. dp.fracture.Wf
	
Wf
	
grid_discretization_DP_model. m
	3
	是
	裂缝缝宽

	
discretization. dp.fracture.Porf
	
Porf
	
grid_discretization_DP_model. m
	3
	是
	裂缝孔隙度

	
discretization. dp.fracture. prporf
	
prporf
	
grid_discretization_DP_model. m
	3
	是
	裂缝参考压力

	
discretization. dp.fracture. cporf
	
cporf
	
grid_discretization_DP_model. m
	3
	是
	裂缝压缩系数

	
discretization. dp.stress. fracture_factor
	
stress_factor_fracture
	
grid_discretization_DP_model. m
	3
	是
	应力敏感

	
discretization. dp.stress. matrix_factor
	
stress_factor_matrix
	
grid_discretization_DP_model. m
	3
	是
	应力敏感

	
discretization. dp.stress. ref_pressure
	
stress_factor_ref_pressure
	
grid_discretization_DP_model. m
	3
	是
	参考压力




	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
discretization. dp.rock_density
	
rock_density
	
grid_discretization_DP_model. m
	3
	是
	岩石密度

	
discretization. dp.Rpt
	
Rpt
	
grid_discretization_DP_model. m
	3
	是
	含义待进一步确认

	
discretization. dp.cf
	
cf
	
grid_discretization_DP_model. m
	3
	是
	含义待进一步确认

	
discretization. dp.ca
	
ca
	
grid_discretization_DP_model. m
	3
	是
	含义待进一步确认



[bookmark: Flow: Gas-Water]Flow: Gas-Water

	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
flow.gas_water.gas_prop.VL
	
gas_prop.VL
	
gas_water_flow. m
	4
	是
	Langmuir 体积

	
flow.gas_water.gas_prop.PL
	
gas_prop.PL
	
gas_water_flow. m
	4
	是
	Langmuir 压力

	
flow.gas_water.gas_prop.Kn
	
gas_prop.Kn
	
gas_water_flow. m
	4
	是
	Knudsen 数

	
flow.gas_water.gas_prop. Kn_modified_factor
	
gas_prop. Kn_modified_factor
	
gas_water_flow. m
	4
	否
	派生值

	
flow.gas_water.gas_prop. beta_non_darcy_flow
	
gas_prop. beta_non_Darcy_flow
	
gas_water_flow. m
	4
	是
	高速流修正项

	
flow.gas_water. p_grad_threshold
	
p_grad_threshold
	
gas_water_flow. m
	4
	是
	启动压力梯度



	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
flow.gas_water.density_g_sc
	
density_g_sc
	
gas_water_flow. m
	4
	是
	标况气体密度

	
flow.gas_water.density_w_sc
	
density_w_sc
	
gas_water_flow. m
	4
	是
	标况水密度

	
flow.gas_water.gas_model
	
gas_model
	
gas_water_flow. m
	4
	是
	1 生成型 PVT，
2 表格型 PVT

	
flow.gas_water.prg
	
prg
	
gas_water_flow. m
	4
	是
	仅在模型 1 中使用

	
flow.gas_water.Bgi
	
Bgi
	
gas_water_flow. m
	4
	是
	仅在模型 1 中使用

	
flow.gas_water.cg
	
cg
	
gas_water_flow. m
	4
	是
	仅在模型 1 中使用

	
flow.gas_water.vgi
	
vgi
	
gas_water_flow. m
	4
	是
	仅在模型 1 中使用

	
flow.gas_water.cvg
	
cvg
	
gas_water_flow. m
	4
	是
	仅在模型 1 中使用

	
flow.gas_water.Ppr
	
Ppr
	
gas_water_flow. m
	4
	是
	表格或生成值

	
flow.gas_water.BG
	
BG
	
gas_water_flow. m
	4
	是
	表格或生成值

	
flow.gas_water.MUG
	
MUG
	
gas_water_flow. m
	4
	是
	表格或生成值

	
flow.gas_water.prw
	
prw
	
gas_water_flow.
	4
	是
	水参考压力




	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
	
	
m
	
	
	

	
flow.gas_water.Bwi
	
Bwi
	
gas_water_flow. m
	4
	是
	水体积系数

	
flow.gas_water.cw
	
cw
	
gas_water_flow. m
	4
	是
	水压缩系数

	
flow.gas_water.vwi
	
vwi
	
gas_water_flow. m
	4
	是
	水黏度

	
flow.gas_water.cvw
	
cvw
	
gas_water_flow. m
	4
	是
	水黏压系数

	
flow.gas_water.ifpcgl
	
ifpcgl
	
gas_water_flow. m
	4
	是
	毛管压开关

	
flow.gas_water. matrix_relperm_table
	
RPGW
	
gas_water_flow. m
	4
	是
	基质相对渗透率表

	
flow.gas_water. fracture_relperm_table
	
PRF
	
gas_water_flow. m
	4
	是
	裂缝相对渗透率表



[bookmark: Flow: Oil-Water]Flow: Oil-Water

	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
flow.oil_water.density_o_sc
	
density_o_sc
	
oil_water_flow. m
	5,6,7
	是
	原油密度

	
flow.oil_water.density_w_sc
	
density_w_sc
	
oil_water_flow. m
	5,6,7
	是
	水密度

	
flow.oil_water.oil_model
	
oil_model
	
oil_water_flow.
	5,6,7
	是
	1 生成型 PVT，
2 表格型



	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
	
	
m
	
	
	

	
flow.oil_water.pro
	
pro
	
oil_water_flow. m
	5,6,7
	是
	原油参考压力

	
flow.oil_water.Boi
	
Boi
	
oil_water_flow. m
	5,6,7
	是
	原油体积系数

	
flow.oil_water.co
	
co
	
oil_water_flow. m
	5,6,7
	是
	原油压缩系数

	
flow.oil_water.voi
	
voi
	
oil_water_flow. m
	5,6,7
	是
	原油黏度

	
flow.oil_water.cvo
	
cvo
	
oil_water_flow. m
	5,6,7
	是
	原油黏压系数

	
flow.oil_water.Ppr
	
Ppr
	
oil_water_flow. m
	5,6,7
	是
	表格或生成值

	
flow.oil_water.BO
	
BO
	
oil_water_flow. m
	5,6,7
	是
	表格或生成值

	
flow.oil_water.MUO
	
MUO
	
oil_water_flow. m
	5,6,7
	是
	表格或生成值

	
flow.oil_water.prw
	
prw
	
oil_water_flow. m
	5,6,7
	是
	水参考压力

	
flow.oil_water.Bwi
	
Bwi
	
oil_water_flow. m
	5,6,7
	是
	水体积系数

	
flow.oil_water.cw
	
cw
	
oil_water_flow. m
	5,6,7
	是
	水压缩系数




	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
flow.oil_water.vwi
	
vwi
	
oil_water_flow. m
	5,6,7
	是
	水黏度

	
flow.oil_water.cvw
	
cvw
	
oil_water_flow. m
	5,6,7
	是
	水黏压系数

	
flow.oil_water.ifpcow
	
ifpcow
	
oil_water_flow. m
	5,6,7
	是
	毛管压开关

	
flow.oil_water. matrix_relperm_table
	
PRM
	
oil_water_flow. m
	5,6,7
	是
	基质表

	
flow.oil_water. fracture_relperm_table
	
PRF
	
oil_water_flow. m
	5,6,7
	是
	裂缝表

	
flow.oil_water. beta_non_darcy_flow
	
beta_non_Darcy_flow
	
oil_water_flow. m
	5,6,7
	是
	非达西系数

	
flow.oil_water. p_grad_threshold
	
p_grad_threshold
	
oil_water_flow. m
	5,6,7
	是
	启动梯度



[bookmark: Flow: Multi-Component]Flow: Multi-Component

	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
flow.multi_component.Ds
	
Ds
	
multi_component_flow. m
	1,2,3
	是
	表活扩散系数
	

	
flow.multi_component.Db
	
Db
	
multi_component_flow. m
	1,2,3
	是
	盐扩散系数

	
flow.multi_component. c_ca_table
	
c_ca_table
	
multi_component_flow. m
	1,2,3
	是
	吸附表
	



	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
flow.multi_component. cs_data
	
cs_data
	
multi_component_flow. m
	1,2,3
	否
	由表派生

	
flow.multi_component. cb_data
	
cb_data
	
multi_component_flow. m
	1,2,3
	否
	由表派生
	

	
flow.multi_component. csa_data
	
csa_data
	
multi_component_flow. m
	1,2,3
	否
	由表派生

	
flow.multi_component. cba_data
	
cba_data
	
multi_component_flow. m
	1,2,3
	否
	由表派生
	

	
flow.multi_component.R
	
R
	
multi_component_flow. m
	1,2,3
	是
	化学常数

	
flow.multi_component.Vm
	
Vm
	
multi_component_flow. m
	1,2,3
	是
	摩尔体积
	

	
flow.multi_component. Temperature
	
Temperature
	
multi_component_flow. m
	1,2,3
	是
	温度

	
flow.multi_component. chemistry_cof
	
chemistry_cof
	
multi_component_flow. m
	1,2,3
	否
	派生值
	

	
flow.multi_component. x_matrix!!!!
	
xm
	
multi_component_flow. m
	1,2,3
	是
	基质单元化学活度因子

	
flow.multi_component. x_fracture!!!
	
xf
	
multi_component_flow. m
	1,2,3
	是
	裂缝单元化学活度因子
	

	
flow.multi_component. cs_Nc
	
cs_Nc
	
multi_component_flow. m
	1,2,3
	是
	动态相对渗透率映射

	
flow.multi_component. Nc_nosurf
	
Nc_nosurf
	
multi_component_flow.
	1,2,3
	否
	派生值
	




	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
	
	
m
	
	
	
	

	
flow.multi_component. Nc_surf
	
Nc_surf
	
multi_component_flow. m
	1,2,3
	否
	派生值

	
flow.multi_component. kr_nosurf
	
kr_nosurf
	
multi_component_flow. m
	1,2,3
	是
	相对渗透率表
	

	
flow.multi_component. kr_surf
	
kr_surf
	
multi_component_flow. m
	1,2,3
	是
	相对渗透率表

	
flow.multi_component.PC
	
PC
	
multi_component_flow. m
	1,2,3
	是
	毛管压表
	

	
flow.multi_component. cs_Nc_fracture
	
cs_Nc_fracture
	
multi_component_flow. m
	1,2,3
	是
	裂缝表

	
flow.multi_component. kr_nosurf_fracture
	
kr_nosurf_fracture
	
multi_component_flow. m
	1,2,3
	是
	裂缝表
	

	
flow.multi_component. kr_surf_fracture
	
kr_surf_fracture
	
multi_component_flow. m
	1,2,3
	是
	裂缝表

	
flow.multi_component. PC_fracture
	
PC_fracture
	
multi_component_flow. m
	1,2,3
	是
	裂缝毛管压表
	

	
flow.multi_component. ifpcgl
	
ifpcgl
	
multi_component_flow. m
	1,2,3
	是
	毛管压开关

	
flow.multi_component. p_grad_threshold
	
p_grad_threshold
	
multi_component_flow. m
	1,2,3
	是
	启动梯度
	

	
flow.multi_component. gas_prop.VL
	
gas_prop.VL
	
multi_component_flow. m
	1,2,3
	是
	类油场景中通常为0




	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
flow.multi_component. gas_prop.PL
	
gas_prop.PL
	
multi_component_flow. m
	1,2,3
	是
	Langmu 压力
	

	
flow.multi_component. gas_prop.Kn
	
gas_prop.Kn
	
multi_component_flow. m
	1,2,3
	是
	Knudsen 数

	
flow.multi_component. gas_prop.
Kn_modified_factor
	
gas_prop. Kn_modified_factor
	
multi_component_flow. m
	1,2,3
	否
	派生值
	

	
	
gas_prop. stress_factor_fracture
	
multi_component_flow. m
	1,2,3
	是
	在算例流体文件中出现

	
flow.multi_component. gas_prop. stress_factor_matrix
	
gas_prop. stress_factor_matrix
	
multi_component_flow. m
	1,2,3
	是
	在算例流体文件中出现
	

	
flow.multi_component. gas_prop. stress_factor_ref_pressure
	
gas_prop. stress_factor_ref_pressure
	
multi_component_flow. m
	1,2,3
	是
	在算例流体文件中出现

	
flow.multi_component. gas_prop. beta_non_darcy_flow
	
gas_prop. beta_non_Darcy_flow
	
multi_component_flow. m
	1,2,3
	是
	非达西系数
	

	
flow.multi_component. density_g_sc
	
density_g_sc
	
multi_component_flow. m
	1,2,3
	是
	标况密度

	
flow.multi_component. gas_model
	
gas_model
	
multi_component_flow. m
	1,2,3
	是
	1 生成型，2 表格型
	

	
flow.multi_component.prg
	
prg
	
multi_component_flow. m
	1,2,3
	是
	参考压力

	
flow.multi_component.Bgi
	
Bgi
	
multi_component_flow. m
	1,2,3
	是
	体积系数
	

	
flow.multi_component.cg
	
cg
	
	1,2,3
	是
	压缩系数


 (
flow.multi_component.
gas_prop.
stress_factor_fracture
)

	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
	
	
multi_component_flow. m
	
	
	

	
flow.multi_component.vgi
	
vgi
	
multi_component_flow. m
	1,2,3
	是
	黏度
	

	
flow.multi_component.cvg
	
cvg
	
multi_component_flow. m
	1,2,3
	是
	黏压系数

	
flow.multi_component.Ppr
	
Ppr
	
multi_component_flow. m
	1,2,3
	是
	表格或生成值
	

	
flow.multi_component.BG
	
BG
	
multi_component_flow. m
	1,2,3
	是
	表格或生成值

	
flow.multi_component.MUG
	
MUG
	
multi_component_flow. m
	1,2,3
	是
	表格或生成值
	

	
flow.multi_component. density_w_sc
	
density_w_sc
	
multi_component_flow. m
	1,2,3
	是
	水密度

	
flow.multi_component.prw
	
prw
	
multi_component_flow. m
	1,2,3
	是
	水参考压力
	

	
flow.multi_component.Bwi
	
Bwi
	
multi_component_flow. m
	1,2,3
	是
	水体积系数

	
flow.multi_component.cw
	
cw
	
multi_component_flow. m
	1,2,3
	是
	水压缩系数
	

	
flow.multi_component.vwi
	
vwi
	
multi_component_flow. m
	1,2,3
	是
	水黏度

	
flow.multi_component.cvw
	
cvw
	
multi_component_flow. m
	1,2,3
	是
	水黏压系数
	




	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
flow.multi_component. number_state_variables
	
number_state_variables
	
multi_component_flow. m
	1,2,3
	否
	当前代码固定为 4



[bookmark: Initial Conditions]Initial Conditions

	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
initial.pressure
	
P
	flow files
	1-7
	是
	初始压力数组

	
initial.sw
	
Sw
	flow files
	1-7
	是
	初始含水饱和度数组

	
initial.cs
	
Cs
	
multi_component_flow.m
	1,2,3
	是
	初始表活浓度

	
initial.cb
	
Cb
	
multi_component_flow.m
	1,2,3
	是
	初始盐浓度


[bookmark: Wells]Wells

	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
wells.well1
	
well1
	
main1.m
	1-7
	是
	常规井表

	
wells.num_fracture_wells
	
num_fracture_wells
	
main1.m
	1-7
	是
	数量

	
wells.welloc
	
welloc
	
main1.m
	1-7
	是
	压裂井坐标

	
wells.perfnum
	
perfnum
	helper 输出
	1-7
	否
	由 findWelloc 推 导

	
wells.well2
	
well2
	
main1.m
	1-7
	是
	压裂井表

	
wells.Wellc
	
Wellc
	helper 输出
	1-7
	否
	运行期组合结构


常规井单行结构： 井名
射孔数
射孔网格索引矩阵井筒半径
skin 井类型

压裂井单行结构：

井名射孔数
射孔索引井筒半径skin
井类型

[bookmark: Schedule]Schedule

	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
schedule.number_phases
	
number_phases
	
main1.m
	1-7
	是
	阶段数

	
schedule.well_schedules
	
well_schedules
	
main1.m
	1-7
	是
	每个阶段的控制行

	
schedule.time
	
time
	
main1.m
	1-7
	是
	阶段时长向量

	
schedule.dtmax
	
dtmax
	
main1.m
	1-7
	是
	各阶段最大时间步

	
schedule.dtmin
	
dtmin
	
main1.m
	1-7
	是
	各阶段最小时间步


观察到的 schedule 单行字段： 井名
井状态井角色控制模式目标值 1
目标值 2

[bookmark: Solver]Solver

	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
solver.yitap
	
yitap
	
main1.m
	1-7
	是
	自适应时间步控制

	
solver.yitas
	
yitas
	
main1.m
	1-7
	是
	自适应时间步控制

	
solver.omega
	
omega
	
main1.m
	1-7
	是
	自适应时间步控制

	
solver.Nmax
	
Nmax
	
main1.m
	1-7
	是
	牛顿最大迭代次数



	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
solver.epsave
	
epsave
	
main1.m
	1-7
	是
	平均残差容限

	
solver.epsmax
	
epsmax
	
main1.m
	1-7
	是
	最大残差容限



[bookmark: Runtime / Output]Runtime / Output

	Config Path
	Source Variable
	Source File
	Cases
	Editable
	Notes

	
output.result_name
	无
	未来 GUI
	全部
	是
	结果标签

	
output.save_input_path
	无
	未来 GUI
	全部
	是
	输入保存位置

	
output.save_result_path
	无
	未来 GUI
	全部
	是
	结果保存位置

	
output.plot_requests
	无
	未来 GUI
	全部
	是
	用户请求的绘图动作


仅运行期输出：

	Times
	

	OutputRs

	Wellpara

	trun
	



[bookmark: 已知需要统一的地方]
[bookmark: _GoBack]



